# LIVE WEIGHING

In the Live View mode you can see all connected scales.
The weight of up to 10 scales is displayed live.
The axle weight always adds up two scales (axle 1 = scales 1 + 2, axle 2 = scales 3 + 4, ...). The total weight is the sum of all scales.
If you have connected several weighing systems (several radio receivers), you can select the desired weighing system at the top right (blue box with number).

# CENTER OF GRAVITY

In the Center of Gravity mode, you can determine the center of gravity and weight distribution of a vehicle. For this mode you need at least four connected scales (addr. 1-4). If you have connected more scales, only the first four scales (addr. 1-4) are used for this mode.

# CORNER BALANCE

Corner balancing is the process of shifting the weight carried by each wheel to approach optimal values. Although some weight can be shifted between wheels by physically relocating parts of the car, the corner balance process is focused on shifting weight by adjusting the suspension spring height. Any relocation of parts should be performed before corner balancing begins.

# AXLE WEIGHING

In the Axle Weighing mode you can save the weight of up to {max_axles} axles.
For this mode you need at least two connected scales (addr. 1-2). If you have connected more scales, only the first two scales (addr. 1-2) are used for this mode.
You can have the axle weight recorded manually or automatically.
If the weight is recorded automatically, you must set the vehicle type under Settings / Parameters / Parameters for axle weighing (car / truck).
Select the setting “car” for car scales and the setting “truck” for truck scales.

# SAVE

You can save the weighing result immediately from any mode.
Please enter at least one clear vehicle information when entering the customer data.
The test reports can be found under Reports and in the program root directory as PDF file.

# REPORTS

Here you can find the saved test reports. These can be opened, printed and deleted.

# SETTINGS

You will find the following menu items under Settings: Language, Units, User Data, Parameters.

- Language: you can set the program language
- Units: you can set the physical weight unit [kg] or [lb]
- User Data: you can save the operator data and your company logo for the test reports
- Parameters: you can set parameters for the automatic axle weighing, select the connected weighing system and change the radio channel of the radio receiver.

For further Information about scales and accessories please see the operation manual and datasheets.